|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Code** | **Code (old)** | **HCD Name** | **SM Name** | **NAP SubType**  | **Data Type** |
| 1 | 1 | HCD\_Machine\_Type\_Model | HealthMachineTypeModel | 1 | String |
| 2 | 2 | HCD\_Firmware\_Name | HealthFirmware:FirmwareName | 2 | String |
| 3 | 3 | HCD\_Vendor\_Name | HealthVendorName | 3 | String |
| 4 | 4 | HCD\_Vendor\_SMI\_Code | HealthVendorSMICode | 4 | Integer |
| 5 | 5 | HCD\_Firmware\_Version | HealthFirmware:FirmwareVersion | 5 | OctetArray|base64Binary |
| 6 | 6 | HCD\_Firmware\_Patches | HealthFirmware:FirmwarePatches | 6 | String |
| 7 | 20 | HCD\_Firmware\_String\_Version | HealthFirmware:FirmwareStringVersion | 20 | String |
| 8 |  | HCD\_User\_Application\_Enabled | HealthUserApplicationEnabled |  | Boolean |
| 9 |  | HCD\_User\_Application\_Persistence\_Enabled | HealthUserApplicationPersistenceEnabled |  | Boolean |
| 10 | 7 | HCD\_User\_Application\_Name | UserApplicationName | 7 | String |
| 11 | 8 | HCD\_User\_Application\_Version | UserApplicationVersion | 8 | OctetArray|base64Binary |
| 12 | 9 | HCD\_User\_Application\_Patches | UserApplicationPatches | 9 | String |
| 13 | 21 | HCD\_User\_Application\_String\_Version | UserApplicationStringVersion | 21 | String |
| 14 | 10 | HCD\_Resident\_Application\_Name | HealthResidentApplication:ResidentApplicationName | 10 | String |
| 15 | 11 | HCD\_Resident\_Application\_Version | HealthResidentApplication:ResidentApplicationVersion | 11 | OctetArray|base64Binary |
| 16 | 12 | HCD\_Resident\_Application\_Patches | HealthResidentApplication:ResidentApplicationPatches | 12 | String |
| 17 | 22 | HCD\_Resident\_Application\_String\_Version | HealthResidentApplication:ResidentApplicationStringVersion | 22 | String |
| 18 | 13 | HCD\_Firewall\_Setting | HealthFirewallSetting | 13 | OctetArray|base64Binary |
| 19 | 14 | HCD\_Certification\_State | HealthCertificationState | 14 | OctetArray|base64Binary |
| 20 | 15 | HCD\_Configuration\_State | HealthConfigurationState | 15 | OctetArray|base64Binary |
| 21 | 16 | HCD\_Forwarding\_Enabled | HealthForwardingEnabled | 16 | Boolean |
| 22 | 17 | HCD\_PSTN\_Fax\_Enabled | HealthPSTNFaxEnabled | 17 | Boolean |
| 23 | 18 | HCD\_Default\_Password\_Enabled | HealthDefaultPasswordEnabled | 18 | Boolean |
| 24 | 19 | HCD\_Time\_Source | HealthTimeSource | 19 | String |
|  | 23 | HCD\_Configuration\_Flags 1 |  | 23 | OctetArray|base64Binary |
| 25 | 24 | HCD\_Attribute\_Natural\_Language | NaturalLanguageConfigured | 24 | String |

1 HCD\_Configuration\_Flags added in August 2008 to combine HCD\_Forwarding\_Enabled, HCD\_Default\_Password\_Enabled, and HCD\_PSTN\_Fax\_Enabled into a single bitmao, but to also add additional information on not just the state value of the attribute, but whether the attribute feature is supported or not.